# Containerize Network Function Over BareMetal Servers and Infrastructure Slicing

* Textbook definition for 5G slicing is that "5G network slicing is a network architecture that enables the multiplexing of virtualized and independent logical networks on the same physical network infrastructure. Each network slice is an isolated end-to-end network tailored to fulfil diverse requirements requested by a particular application."

## Problem Statement

* How network slicing can be achieved in NFVI (Network Function Virtualization Infrastructure).
  + NFVI slicing is easier to achieve once Containerized Network Function (CNF) PODs are running over the Infrastructure as a Service virtual machines (VMs).
  + There is strong advocacy from a school of thought that CNF PODs should run on bare metal servers (BMS).
  + Running CNF PODs over BMS can solve issues related to performance overhead and networking complexities can also be avoided which are inherited when CNI must run POD networks inside the IaaS VMs.
* If CNF Pods must be run on BMS then it means one BMS will be used as single k8s worker node which is clearly underutilization of compute resource.

## Use cases for Running CNF over BMS

* In 5G Cloud-RAN DU (distribution unit) is deployed near to RU (Radio Unit) as low latency is required for DU.
  + Cloud-native DU workloads require low latency thus requires BMS based K8s deployment.
  + Using a BMS; only to host single k8s node is clearly under-utilization of compute resources.
* In 5G Cloud-RAN CU (Central unit) is deployed far away from Radio Unit (RU) and can bear some latency, but it is still desirable to keep the latency to minimum effect.
* In 5G Core Control plane sites, compute resources are usually shared to run following applications.
  + Policy Control Function
  + Packet Core Controller
  + IMS control plane components
* In 5G Core user plane sites, compute resources are usually shared to run following applications.
  + Packet Core Gateway (5G Core User plane)
  + IMS transport and bearer services (user plane)
  + DNS services
* All above-described use cases requires that CNF Pods should get performance as those are running over BMS, but compute resources should not be underutilized by dedicating the one BMS to a single K8s worker node.
  + Above implies that we need slicing of compute resources while still offering bare metal performance to CNF Pods.

## Proposed Model - BMS Slicing using Hardware Pass-through technology from Bare Metal to the Guest VMs

* BMS slicing means avoiding Qemu emulation of CPUs for Guest VMs (k8s worker nodes) and extending network devices either as PCI-Passthrough or SRIOV VF.
* If k8s is deployed on BMS sliced infrastructure, then following problems would be resolved: -
  + No more under-utilization of compute infrastructure as one BMS is not limited to host one k8s worker node.
  + Same level of performance as if k8s worker nodes is deployed over BMS or inside Guest VMs which is sliced from BMS.
  + No networking complexities, which are inherent if k8s worker nodes have to be deployed over IaaS VMs.

A picture containing text, screenshot, font, diagram

Description automatically generated

* Slice your bare metal server (get requirements for VM/ VMs CPU, Memory and required NICs).
  + Define the VM / VMs on your bare metal server (without running the VM).
  + Define number of CPUs, map the vCPUs to Host (bare metal) CPUs.
  + While defining the vCPUs, use the "host-pass-through" CPU model".
  + Add vCPUs for Emulator threads and IOThreads.
  + Identify the NICs (PCI) on bare metal servers which should be passthrough to VMs.
  + Detach the NIC (PCI) from the Host (bare metal) and attach it to the Guest VMs.
  + Isolate the CPUs Cores allocated to VMs, IOThreads and Emulator Threads from the Host (bare metal) OS.
  + This model will ensure that bare metal performance can be achieved for CNF PODS running inside the VMs and network complexities are also reduced.

## Implementation Details

* Most of above-described requirements can be achieved via IaaS (Open stack, but I will not discuss that).
* I will discuss implementation details for Host OS (Ubuntu 18.04) and Guest VMs Running (Centos 18.06).
  + Identify the NUMA Architecture

server1:~$ lscpu

Architecture: x86\_64

CPU op-mode(s): 32-bit, 64-bit

Byte Order: Little Endian

CPU(s): 24

On-line CPU(s) list: 0-23

Thread(s) per core: 2

Core(s) per socket: 6

Socket(s): 2

NUMA node(s): 2

Vendor ID: GenuineIntel

CPU family: 6

Model: 62

Model name: Intel(R) Xeon(R) CPU E5-2620 v2 @ 2.10GHz

Stepping: 4

CPU MHz: 1200.529

CPU max MHz: 2600.0000

CPU min MHz: 1200.0000

BogoMIPS: 4199.96

Virtualization: VT-x

L1d cache: 32K

L1i cache: 32K

L2 cache: 256K

L3 cache: 15360K

NUMA node0 CPU(s): 0,2,4,6,8,10,12,14,16,18,20,22

NUMA node1 CPU(s): 1,3,5,7,9,11,13,15,17,19,21,23

server1:~$ sudo cat $(find /sys/devices/system/cpu -regex ".\*cpu[0-9]+/topology/thread\_siblings\_list") | sort -n | uniq

0,12

1,13

2,14

3,15

4,16

5,17

6,18

7,19

8,20

9,21

10,22

11,23

* I have 2 socket machine each with 6 physical cores and enabling hyperthreading gave me 12 cores on each socket, but each CPU sibling will be dedicated to the purpose for which main core will be used.
* Host OS CPU Cores

0,12

1,13

* Guest VM - Red\_k8s\_cluster\_worker1

2,14 Physical CPUs mapped to Emulator threads and IOThreads

4,16 Physical CPUs Mapped to Guest VM vCPUs

6,18

8,20

10,22

* Guest VM - Red\_k8s\_cluster\_worker1

3,15 Physical CPUs mapped to Emulator threads and IOThreads

5,17 Physical CPUs Mapped to Guest VM vCPUs

7,19

9,21

11,23

* Isolate the CPUs so that host OS scheduler should not use CPUs dedicated for Guest VMs, Emulator Threads and Guest IOThread.
* Enable pci-pass-through and CPU Isolation in Grub config.

vim /etc/default/grub

GRUB\_CMDLINE\_LINUX="intel\_iommu=on isolcpus=2-11,14-23"

update-grub

shutdown -r now

* Verify if the IOMMU is enabled or not

root@server1:/tmp# dmesg | grep IOMMU

[ 0.000000] DMAR: IOMMU enabled

[ 0.000000] DMAR-IR: IOAPIC id 2 under DRHD base 0xd0100000 IOMMU 0

[ 0.000000] DMAR-IR: IOAPIC id 0 under DRHD base 0xdc100000 IOMMU 1

[ 0.000000] DMAR-IR: IOAPIC id 1 under DRHD base 0xdc100000 IOMMU 1

* Identify the NICs which will be passed through to the Guest VMs.

sudo lshw -c network -businfo

Bus info Device Class Description

========================================================

pci@0000:01:00.0 eno1 network Ethernet Controller 10-Gigabit X540-AT2

pci@0000:01:00.1 eno2 network Ethernet Controller 10-Gigabit X540-AT2

pci@0000:08:00.0 eno3 network I350 Gigabit Network Connection

pci@0000:08:00.1 eno4 network I350 Gigabit Network Connection

virbr0 network Ethernet interface

* I will utilize eno1 and eno2 as PCI passthrough devices.

virsh nodedev-dumpxml pci\_0000\_01\_00\_0

<device>

<name>pci\_0000\_01\_00\_0</name>

<path>/sys/devices/pci0000:00/0000:00:01.0/0000:01:00.0</path>

<parent>pci\_0000\_00\_01\_0</parent>

<driver>

<name>vfio-pci</name>

</driver>

<capability type='pci'>

<domain>0</domain>

<bus>1</bus>

<slot>0</slot>

<function>0</function>

<product id='0x1528'>Ethernet Controller 10-Gigabit X540-AT2</product>

<vendor id='0x8086'>Intel Corporation</vendor>

<capability type='virt\_functions' maxCount='63'/>

<iommuGroup number='25'>

<address domain='0x0000' bus='0x01' slot='0x00' function='0x0'/>

</iommuGroup>

<numa node='0'/>

<pci-express>

<link validity='cap' port='0' speed='5' width='8'/>

<link validity='sta' speed='5' width='8'/>

</pci-express>

</capability>

</device>

virsh nodedev-dumpxml pci\_0000\_01\_00\_1

<device>

<name>pci\_0000\_01\_00\_1</name>

<path>/sys/devices/pci0000:00/0000:00:01.0/0000:01:00.1</path>

<parent>pci\_0000\_00\_01\_0</parent>

<driver>

<name>vfio-pci</name>

</driver>

<capability type='pci'>

<domain>0</domain>

<bus>1</bus>

<slot>0</slot>

<function>1</function>

<product id='0x1528'>Ethernet Controller 10-Gigabit X540-AT2</product>

<vendor id='0x8086'>Intel Corporation</vendor>

<capability type='virt\_functions' maxCount='63'/>

<iommuGroup number='26'>

<address domain='0x0000' bus='0x01' slot='0x00' function='0x1'/>

</iommuGroup>

<numa node='0'/>

<pci-express>

<link validity='cap' port='0' speed='5' width='8'/>

<link validity='sta' speed='5' width='8'/>

</pci-express>

</capability>

</device>

* Detach the selected PCI Devices from Host OS (Bare Metal Server)

virsh nodedev-detach pci\_0000\_01\_00\_0

virsh nodedev-detach pci\_0000\_01\_00\_1

lshw -c network -businfo

Bus info Device Class Description

========================================================

pci@0000:01:00.0 network Ethernet Controller 10-Gigabit X540-AT2

pci@0000:01:00.1 network Ethernet Controller 10-Gigabit X540-AT2

pci@0000:08:00.0 eno3 network I350 Gigabit Network Connection

pci@0000:08:00.1 eno4 network I350 Gigabit Network Connection

virbr0 network Ethernet interface

virbr0-nic network Ethernet interface

* Create Guest VMs Definition Files
* Red\_k8s\_cluster\_worker1 VM

node\_name=Red\_k8s\_cluster\_worker1

export LIBGUESTFS\_BACKEND=direct

root\_password=root-password

someuser\_password=someuser-password

cloud\_image=/var/lib/libvirt/images/CentOS-7-x86\_64-GenericCloud-1811.qcow2

qemu-img create -f qcow2 /var/lib/libvirt/images/${node\_name}.qcow2 100G

virt-resize --expand /dev/sda1 ${cloud\_image} /var/lib/libvirt/images/${node\_name}.qcow2 && virt-customize -a /var/lib/libvirt/images/${node\_name}.qcow2 --run-command 'xfs\_growfs /' --selinux-relabel

virt-customize -a /var/lib/libvirt/images/${node\_name}.qcow2 --run-command 'xfs\_growfs /' --root-password password:${root\_password} --hostname ${node\_name}.${nodesuffix} --run-command 'useradd someuser' --password someuser:password:${someuser\_password} --run-command 'echo "someuser ALL=(root) NOPASSWD:ALL" | tee -a /etc/sudoers.d/someuser' --chmod 0440:/etc/sudoers.d/someuser --run-command 'sed -i "s/PasswordAuthentication no/PasswordAuthentication yes/g" /etc/ssh/sshd\_config' --run-command 'systemctl enable sshd' --run-command 'yum remove -y cloud-init' --selinux-relabel

virt-install --name ${node\_name} \

--virt-type kvm --memory 8192 --vcpus 8 \

--boot hd,menu=on \

--disk path=/var/lib/libvirt/images/${node\_name}.qcow2,device=disk \

--graphics vnc \

--cpu host-passthrough \

--os-type=Linux \

--os-variant=centos7.0 \

--host-device=pci\_0000\_01\_00\_0 \

--console pty,target\_type=serial \

--dry-run --print-xml > /tmp/${node\_name}.xml

* Blue\_k8s\_cluster\_worker1 VM

node\_name=Blue\_k8s\_cluster\_worker1

export LIBGUESTFS\_BACKEND=direct

root\_password=root-password

someuser\_password=someuser-password

cloud\_image=/var/lib/libvirt/images/CentOS-7-x86\_64-GenericCloud-1811.qcow2

qemu-img create -f qcow2 /var/lib/libvirt/images/${node\_name}.qcow2 100G

virt-resize --expand /dev/sda1 ${cloud\_image} /var/lib/libvirt/images/${node\_name}.qcow2 && virt-customize -a /var/lib/libvirt/images/${node\_name}.qcow2 --run-command 'xfs\_growfs /' --selinux-relabel

virt-customize -a /var/lib/libvirt/images/${node\_name}.qcow2 --run-command 'xfs\_growfs /' --root-password password:${root\_password} --hostname ${node\_name}.${nodesuffix} --run-command 'useradd someuser' --password someuser:password:${someuser\_password} --run-command 'echo "someuser ALL=(root) NOPASSWD:ALL" | tee -a /etc/sudoers.d/someuser' --chmod 0440:/etc/sudoers.d/someuser --run-command 'sed -i "s/PasswordAuthentication no/PasswordAuthentication yes/g" /etc/ssh/sshd\_config' --run-command 'systemctl enable sshd' --run-command 'yum remove -y cloud-init' --selinux-relabel

virt-install --name ${node\_name} \

--virt-type kvm --memory 8192 --vcpus 8 \

--boot hd,menu=on \

--disk path=/var/lib/libvirt/images/${node\_name}.qcow2,device=disk \

--graphics vnc \

--cpu host-passthrough \

--os-type=Linux \

--os-variant=centos7.0 \

--host-device=pci\_0000\_01\_00\_1 \

--console pty,target\_type=serial \

--dry-run --print-xml > /tmp/${node\_name}.xml

* Edit the Guest VM definition ffviles.
* Repeat it for both/ all the guest VMs.

vim /tmp/Red\_k8s\_cluster\_worker1.xml

* Remove following line.

<vcpu>8</vcpu>

* Add following line.

<vcpu placement='static'>8</vcpu>

* Add following lines.

<iothreads>1</iothreads>

<cputune>

<vcpupin vcpu='0' cpuset='4'/>

<vcpupin vcpu='1' cpuset='6'/>

<vcpupin vcpu='2' cpuset='8'/>

<vcpupin vcpu='3' cpuset='10'/>

<vcpupin vcpu='4' cpuset='16'/>

<vcpupin vcpu='5' cpuset='18'/>

<vcpupin vcpu='6' cpuset='20'/>

<vcpupin vcpu='7' cpuset='22'/>

<emulatorpin cpuset='2,14'/>

<iothreadpin iothread='1' cpuset='2,14'/>

</cputune>

* Remove following lines.

<interface type="network">

<source network="default"/>

<mac address="52:54:00:13:c2:8e"/>

<model type="virtio"/>

</interface>

* Ensure network devices is added as PCI-Pass-through

<hostdev mode="subsystem" type="pci" managed="yes">

<source>

<address domain="0" bus="1" slot="0" function="0"/>

</source>

</hostdev>

* Define guest VMs

virsh define /tmp/Red\_k8s\_cluster\_worker1.xml

virsh define /tmp/Blue\_k8s\_cluster\_worker1.xml

* Start the guest VMs.

virsh start Red\_k8s\_cluster\_worker1

virsh start Blue\_k8s\_cluster\_worker1

## Verification

* Verify the Network Connectivity between Guest VMs and Underlay\_Fabric\_Switch.
* Underlay\_Fabric\_Switch ports must be configured with correct VLAN on interfaces connected with (bare metal NICs which are passed through to the Guest VMs).
* Once correct config will be applied on Guest VM NICs then connectivity towards fabric and other VMs on same subnet should be established.

fabric-switch> show ethernet-switching table | match bc:30:5b:f2:87:52

Red\_Tenant\_Network bc:30:5b:f2:87:52 Learn 0 ge-0/0/9.0

fabric-switch> show ethernet-switching table interface ge-0/0/8

Ethernet-switching table: 1 unicast entries

VLAN MAC address Type Age Interfaces

Blue\_Tenant\_Network bc:30:5b:f2:87:50 Learn 4:17 ge-0/0/8.0

* Verify CPU Allocation
* CPU Allocation Design

Red\_k8s\_cluster\_worker1 VM

2,14 (Emultaor threads and IOThreads)

4,16 mapped to Guest VM vCPUs

6,18

8,20

10,22

Blue\_k8s\_cluster\_worker1 VM

3,15 (Emultaor threads and IOThreads)

5,17 Mapped to Guest VM vCPUs

7,19

9,21

11,23

* Output Collected from the Host OS

server1:/tmp# virsh vcpuinfo Red\_k8s\_cluster\_worker1

VCPU: 0

CPU: 4

State: running

CPU time: 28.3s

CPU Affinity: ----y-------------------

VCPU: 1

CPU: 6

State: running

CPU time: 24.6s

CPU Affinity: ------y-----------------

VCPU: 2

CPU: 8

State: running

CPU time: 13.9s

CPU Affinity: --------y---------------

VCPU: 3

CPU: 10

State: running

CPU time: 17.8s

CPU Affinity: ----------y-------------

VCPU: 4

CPU: 16

State: running

CPU time: 10.2s

CPU Affinity: ----------------y-------

VCPU: 5

CPU: 18

State: running

CPU time: 9.8s

CPU Affinity: ------------------y-----

VCPU: 6

CPU: 20

State: running

CPU time: 9.4s

CPU Affinity: ---------------------y--

VCPU: 7

CPU: 22

State: running

CPU time: 7.4s

CPU Affinity: -----------------------y

server1:/tmp# virsh emulatorpin Red\_k8s\_cluster\_worker1

emulator: CPU Affinity

----------------------------------

\*: 2,14

server1:~$ virsh vcpuinfo Blue\_k8s\_cluster\_worker1

VCPU: 0

CPU: 5

State: running

CPU time: 25.4s

CPU Affinity: -----y------------------

VCPU: 1

CPU: 7

State: running

CPU time: 11.8s

CPU Affinity: -------y----------------

VCPU: 2

CPU: 9

State: running

CPU time: 9.9s

CPU Affinity: ---------y--------------

VCPU: 3

CPU: 11

State: running

CPU time: 15.5s

CPU Affinity: -----------y------------

VCPU: 4

CPU: 17

State: running

CPU time: 18.9s

CPU Affinity: -----------------y------

VCPU: 5

CPU: 19

State: running

CPU time: 8.8s

CPU Affinity: -------------------y----

VCPU: 6

CPU: 21

State: running

CPU time: 9.4s

CPU Affinity: ---------------------y--

VCPU: 7

CPU: 23

State: running

CPU time: 7.4s

CPU Affinity: -----------------------y

server1:~$ virsh emulatorpin Blue\_k8s\_cluster\_worker1

emulator: CPU Affinity

----------------------------------

\*: 3,15

## Separate Network for Control and Data Plane

A picture containing text, screenshot, diagram, parallel

Description automatically generated

* In above discussion I have used single network inside K8s worker nodes for red and blue cluster.
* If multiple network interfaces are required for each worker node for each K8s cluster, then extend it to the Guest VMs accordingly.

## SRIOV Vs PCI-Passthrough

* SRIOV VFs can be passed to the Guest VFs instead of PCI Passthrough.
* Upside for using SRIOV VFs is that with fewer physical NICs we can provide direct connectivity to the Guest VM (avoiding virtio drivers).
* Downside of SRIOV VFs is that some of the physical network functionality may not be available over the VFs (e.g. LACP or 802.3 ad bond can't be configured over SRIOV VFs).
* Upside of PCI pass-through is that full network functionality would be available to Guest VMs NICs (e.g LACP or 802.3ad can be configured over PCI pass through NICs).
* Downside of PIC pass-through is extra cost for having separate PCI pass-through NICs for each NUMA node which could suffice the Guest VM requirements.

## Next Step

* I will scale up this infrastructure to 4 bare metal servers (1 Control host and 3 Worker nodes) to run 2 K8s clusters (Red and Blue) while running Juniper Networks Cloud Native CN2 as CNI for those K8s Clusters.

## Conclusion

* We can run multiple k8s cluster in same infrastructure and Guest VMs (k8s worker nodes) will get bare metal like performance because of following factors: -
  + Avoiding the virtio drivers and Qemu Emulation for CPUs (because of Hostpass-through CPU model) and NIC cards (because of PCI pass-through).
  + Having dedicated IOthread cores will offer speedy read/write operations to the disk.
  + Dedicated emulator threads will ensure that all Qemu related tasks for guest VMs will be handled by those dedicated cores.
  + Isolating CPU Cores dedicated for Guest VMs, IOThreads and Emulator threads from Host OS CPU cores will ensure that the Host OS scheduler is not overlapping with Guest VMs resources.

## References

* https://wiki.openstack.org/wiki/LibvirtXMLCPUModel
* https://access.redhat.com/documentation/en-us/red\_hat\_enterprise\_linux/7/html/virtualization\_deployment\_and\_administration\_guide/sect-manipulating\_the\_domain\_xml-cpu\_model\_and\_topology
* https://www.intel.com/content/www/us/en/docs/programmable/683013/current/processor-affinity-or-cpu-pinning.html
* https://access.redhat.com/documentation/en-us/red\_hat\_enterprise\_linux\_openstack\_platform/7/html/instances\_and\_images\_guide/ch-cpu\_pinning